Installation for 6 X 6 Base
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**6 x 6 frames should be no greater than dimension of unit**
Double Unit 6x6 Base: (There will be approximately a 1” overhang of shower on 6x6 Base) 
10 qty. - 5” x 3/8” Galvanized lag bolts 
	Double 46” Units:				Double 36” Units:	
  	2 qty. – 44” Pressure Treated Wood		2 qty. – 34” Pressure Treated Wood
 	2 qty. – 86” Pressure Treated Wood 		2 qty. – 66” Pressure Treated Wood
	10 60lb. bags of 3/8 gravel				8 60lb. bags of 3/8 gravel

Single Unit 6x6 Base: (There will be approximately 1” overhang of shower on 6x6 Base)
8 qty. - 5” x 3/8” Galvanized lag bolts
Single  46” Units:				               Single 36” Units:	
  	4 qty. – 44” Pressure Treated Wood		4 qty. – 34” Pressure Treated Wood
	5 60lb. bags of 3/8 gravel				4 60lb. bags of 3/8 gravel

1. Create a lap joint at 5 ½” in length and 2 ¾” in depth on both ends of each piece of wood.
2. Overlap each cut out connection and fasten with (2) 5” x 3/8” lag bolts.
3. Flip the frame over to ensure a smooth surface for the aluminum frame installation.
4. Dig the wood sub-frame into the ground and make sure it is level and stable around the perimeter. Fill the interior with 3/8” stone for a French drain. * 6x6 base should be FLUSH/LEVEL to pavers or grade. 
5. [image: ][image: ][image: ]PLEASE NOTE* - Unit will overhang 1” on all four sides when installing it to the wood for future pavers or tuck stone or dirt. 
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